<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category></Category>
<Model>NV-VZ14EG/NV-VZ14EGE/NV-VZ14EGM/NV-VZ15B/NV-VZ15EG/NV-VZ15EGE/NV-VZ15EGM/NV-VZ15EN/NV-VZ55EG/NV-VZ55EGM</Model>
<System>ORDER NO. VMD0201004C8</System>
<SubSystem>VHS-C Movie</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0401000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=20 month=Feb year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>NV-VZ14EG/NV-VZ14EGE/NV-VZ14EGM/NV-VZ15B/NV-VZ15EG/NV-VZ15EGE/NV-VZ15EGM/NV-VZ15EN/NV-VZ55EG/NV-VZ55EGM</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>4.1 EMAGENCY DISPLAY</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
nvvz14eg
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0400000000x
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0402000000
</nmlist>
</nameloc>
</Para>
<Para>Whenever some abnomal signal is input to the mechacon CPU, an error number (E01, as an example) is displayed in the electronic view finder.</Para>
<Para>In every error status, such the message as shown below alternately appear over and over.</Para>
<Para><randlist prefix=unorder><item><Para>In an emagency mode, all operations except turning on&sol;off the POWER switch are ineffectual.</Para>
</item>
</randlist>
</Para>
<Para>Example (in case of the error number E01):</Para>
<Figure><graphic boardno="graphic10" reprowid="79.248mm" reprodep="27.263mm" location="internal"></Figure>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.787in">
<colspec colnum="2" colname="2" colwidth="2.756in">
<colspec colnum="3" colname="3" colwidth="1.968in">
<colspec colnum="4" colname="4" colwidth="1.575in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>E.VF</Para>
</entry>
<entry colname="2" align="center"><Para>Symptom</Para>
</entry>
<entry colname="3" align="center"><Para>Mode when observed</Para>
</entry>
<entry colname="4" align="center"><Para>Resulting mode</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="center"><Para>E07</Para>
</entry>
<entry colname="2" align="justify"><Para>Short circuit of capstan MDA</Para>
</entry>
<entry colname="3" align="center"><Para>Power ON</Para>
</entry>
<entry colname="4" align="center"><Para>Power OFF</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>E06</Para>
</entry>
<entry colname="2" align="justify"><Para>CAPSTAN FG input absent</Para>
</entry>
<entry colname="3" align="center"><Para>EDIT</Para>
</entry>
<entry colname="4" align="center"><Para>Power OFF</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>E04</Para>
</entry>
<entry colname="2" align="justify"><Para>DRAM FF input absent</Para>
</entry>
<entry colname="3" align="center"><Para>DRAM rotation</Para>
</entry>
<entry colname="4" align="center"><Para>Power OFF</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>E03</Para>
</entry>
<entry colname="2" align="justify"><Para>SUPPLY REEL FG input absent</Para>
</entry>
<entry colname="3" align="center"><Para>REC, PLAY, SERCH, FF</Para>
</entry>
<entry colname="4" align="center"><Para>UNLOADING&rarr;Power OFF</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>E02</Para>
</entry>
<entry colname="2" align="justify"><Para>Mode control motor retates for more than 10 sec<BR>without shift to next mode</Para>
</entry>
<entry colname="3" align="center"><Para>UNLOADING</Para>
</entry>
<entry colname="4" align="center"><Para>Power OFF</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>E01</Para>
</entry>
<entry colname="2" align="justify"><Para>Mode control motor retates for more than 10 sec<BR>without shift to next mode</Para>
</entry>
<entry colname="3" align="center"><Para>LOADING</Para>
</entry>
<entry colname="4" align="center"><Para>Power OFF</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="center"><Para>E00</Para>
</entry>
<entry colname="2" align="justify"><Para>Overtime the programming transaction</Para>
</entry>
<entry colname="3" align="center"><Para>REC, PLAY</Para>
</entry>
<entry colname="4" align="center"><Para>Power OFF</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
nvvz14eg
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0400000000x
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0402000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
