#

4.1 EMAGENCY DISPLAY

TOP PREVIOUS NEXT

Whenever some abnomal signal is input to the mechacon CPU, an error number (E01, as an example) is displayed in the electronic view finder.

In every error status, such the message as shown below alternately appear over and over.

- In an emagency mode, all operations except turning on/off the POWER switch are ineffectual.

Example (in case of the error number E01):

E.VF | Symptom | Mode when observed | Resulting mode
E07 | Short circuit of capstan MDA | Power ON | Power OFF
E06 | CAPSTAN FG input absent | EDIT | Power OFF
E04 | DRAM FF input absent | DRAM rotation | Power OFF
E03 | SUPPLY REEL FG input absent | REC, PLAY, SERCH, FF | UNLOADING→Power OFF
E02 | Mode control motor retates for more than 10 sec without shift to next mode | UNLOADING | Power OFF
E01 | Mode control motor retates for more than 10 sec without shift to next mode | LOADING | Power OFF
E00 | Overtime the programming transaction | REC, PLAY | Power OFF

TOP PREVIOUS NEXT