#

1.2 FEATURE COMPARISON CHART

TOP PREVIOUS NEXT

| NV-VZ14 | NV-VZ15 | NV-VZ55
EG/EGE/EGM | B/EG/EGE/EGM/EN | EG/EGM
CCD | CCD IMAGE SENSOR | 1/6" | 1/6" | 1/6"
CCD Capacity (Pixels) | 350k(500H) | 350k(500H) | 350k(500H)
LCD MONITOR | Color LCD Monitor | 2.5" | 2.5" | 2.5"
LCD Capacity (Pixels) | 112k | 112k | 112k
B/W-EVF | B/W EVF LCD Monitor | 0.24" | 0.24" | 0.24"
EVF LCD Capacity (Pixels) | 76k | 76k | 76k
SPEED | Recording/Playback mode | SP/LP | SP/LP | SP/LP
LENS | Optical Zoom Ratio | x18 | x18 | x18
DIGITAL ZOOM | ZOOM | x700 | x700 | x700
Battery Charge |  | Using Mainbody | Using Mainbody | Using Mainbody
ACCESSORY | Remote controller | ---- | O | O

TOP PREVIOUS NEXT