#

5.1 DISASSEMBLY PROCEDURES

TOP PREVIOUS NEXT

Flow-Chart for Disassembly Procedure

No. | Item/Part | Fig. | Removal (Screw)
1 | Side Case (L) Unit | Fig.1 | 3-Screws (A) 1-Screw (A’)

Fig.2

1-Screw (B)
1-Screw (C)
1-Screw (D)
1-Screw (E)
2-Screws (F)

Fig.3 | Locking Tab (a) Slightly open the Side Case (L) Unit. Disconnect CN27 and CN9013.
2 | Front Case Unit | Fig.4 | 3-Locking Tabs (b) Disconnect CN8 and CN9031.
3 | Main C.B.A. | Fig.5 | 2-Screw (G) Disconnect the following connectors. CN1, CN2, CN3, CN4, CN5, CN7, CV15, CN16, CN22, CN9012, CN9013, CN9018
4 | Cassette Cover Unit | Fig.6 | 1-Screw (H)
5 | Rear Case Unit | Fig.7 | 1-Screw (K) 2-Locking Tabs (c)
6 | EVF Unit | Fig.8 | 2-Screws (L)
7 | Lens Unit | Fig.9 | 2-Screws (M)
8 | Mechanism Unit | Fig.10 | 2-Screws (N) 3-Screws (O)
Fig.11 | 2-Screws (P) 1-Screws (Q)
9 | Main Frame Unit | Fig.6 | 1-Screw (I) 2-Screws (J)
Fig.12 | 7-Locking Tabs (d)

10

LCD Unit

Fig.13

Remove the Sheet.
3-Screws (R)
1-Screw (S)
1-Screw (T)
2-Screws (U)
Remove the Monitor Assy.

Fig.14

2-Screws (V)
1-Screw (W)
Remove the Monitor Cover.
1-Screw (X)
Disconnect CN7603.
Remove the Monitor C.B.A., Sheet (Reflect), Light Screen, Lamp, Diffusion Sheet, LCD Frame, LCDModule and Shield Case.

Fig.14 | 1-Screw (Y) Remove the Lock Spring and Lock Lever.
11 | Back light Unit | Fig.15 | Remove the Polarization Sheet. Remove the LCD Terminal Rubber and Fluorescent Lump.

Fig.1

Fig.2

Fig.3

Fig.4

Fig.5

Fig.6

Fig.7

Fig.8

Fig.9

Fig.10

Fig.11

Fig.12

Fig.13

Fig.14

Fig.15

TOP PREVIOUS NEXT