<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category></Category>
<Model>NV-VZ14EG/NV-VZ14EGE/NV-VZ14EGM/NV-VZ15B/NV-VZ15EG/NV-VZ15EGE/NV-VZ15EGM/NV-VZ15EN/NV-VZ55EG/NV-VZ55EGM</Model>
<System>ORDER NO. VMD0201004C8</System>
<SubSystem>VHS-C Movie</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0202010000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=20 month=Feb year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>NV-VZ14EG/NV-VZ14EGE/NV-VZ14EGM/NV-VZ15B/NV-VZ15EG/NV-VZ15EGE/NV-VZ15EGM/NV-VZ15EN/NV-VZ55EG/NV-VZ55EGM</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title id="TXT19980904144758">2.2.1 Important</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
nvvz14eg
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0202000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0202020000
</nmlist>
</nameloc>
</Para>
<Para>The wires in this mains lead are coloured in accordance with the following code:</Para>
<Table frame="all" colsep="1" rowsep="1"><Title id="Tbl19980904145330"></Title>
<tgroup cols="2" colsep="1" rowsep="1" align="center"><colspec colnum="1" colname="1" colwidth="0.608in">
<colspec colnum="2" colname="2" colwidth="0.664in">
<tbody><row rowsep="1"><entry colname="1" align="center"><Para>Blue</Para>
</entry>
<entry colname="2" align="center"><Para>Neutral</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="center"><Para>Brown</Para>
</entry>
<entry colname="2" align="center"><Para>Live</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Para>As the colours of the wires in the mains lead of this appliance may not correspond with the coloured markings identifying the terminals in your plug, proceed as follows:</Para>
<Para></Para>
<Para>The wire which is coloured BLUE must be connected to the terminal in the plug which is marked with the letter N or coloured BLACK.</Para>
<Para></Para>
<Para>The wire which is coloured BROWN must be connected to the terminal in the plug which is marked with the letter L or coloured RED.</Para>
<Para></Para>
<Para>Under no circumstances should either of these wires be connected to the earth terminal of the three pin plug, marked with the letter E or the Earth Symbol.</Para>
<Figure><graphic boardno="graphic4" reprowid="30.565mm" reprodep="9.144mm" location="internal"></Figure>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
nvvz14eg
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0202000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0202020000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
