# <- this is for OAD need include the 0x500000(KL),0x400000(RFS),0x900000(MSLIB),0x400000(APP),0x100000(CONFIG) = 23MB in T3

#OAD
#nand erase OAD
ubi part UBI
ubi remove oad
ubi create oad 0x3100000
fatload usb 0 80400000 /Target/image/OAD.ubifs
ubi write 80400000 oad 0x3100000

% <- this is end of file symbol
